Supplement to Doc. 9718 Vol II:

*Handbook on Radio Frequency Spectrum Requirements*

*for Civil Aviation*

(as referenced in Doc 9718, Vol II, Appendix C)

Regional Frequency Allotment Tables

| Frequency | Channel | AFI | APAC | CAR | EUR | MID | SAM |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |
| 118.0000 | 118.005 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.0000 | 118.000 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.0083 | 118.010 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.0167 | 118.015 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.0250 | 118.025 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.0250 | 118.030 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.0333 | 118.035 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.0417 | 118.040 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.0500 | 118.055 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.0500 | 118.050 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.0583 | 118.060 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.0667 | 118.065 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.0750 | 118.080 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.0750 | 118.075 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.0833 | 118.085 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.0917 | 118.090 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1000 | 118.100 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.1000 | 118.105 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1083 | 118.110 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1167 | 118.115 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1250 | 118.125 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.1250 | 118.130 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1333 | 118.135 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1417 | 118.140 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1500 | 118.150 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.1500 | 118.155 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1583 | 118.160 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1667 | 118.165 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1750 | 118.175 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.1750 | 118.180 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1833 | 118.185 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.1917 | 118.190 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2000 | 118.200 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.2000 | 118.205 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2083 | 118.210 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2167 | 118.215 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2250 | 118.230 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2250 | 118.225 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.2333 | 118.235 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2417 | 118.240 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2500 | 118.250 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.2500 | 118.255 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2583 | 118.260 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2667 | 118.265 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2750 | 118.275 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.2750 | 118.280 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2833 | 118.285 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.2917 | 118.290 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3000 | 118.300 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.3000 | 118.305 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3083 | 118.310 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3167 | 118.315 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3250 | 118.330 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3250 | 118.325 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.3333 | 118.335 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3417 | 118.340 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3500 | 118.355 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3500 | 118.350 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.3583 | 118.360 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3667 | 118.365 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3750 | 118.380 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3750 | 118.375 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.3833 | 118.385 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.3917 | 118.390 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4000 | 118.400 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.4000 | 118.405 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4083 | 118.410 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4167 | 118.415 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4250 | 118.425 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.4250 | 118.430 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4333 | 118.435 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4417 | 118.440 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4500 | 118.450 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.4500 | 118.455 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4583 | 118.460 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4667 | 118.465 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4750 | 118.475 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.4750 | 118.480 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4833 | 118.485 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.4917 | 118.490 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5000 | 118.500 | ACC-U | TWR | TWR | TWR, APP | TWR | TWR |
| 118.5000 | 118.505 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5083 | 118.510 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5167 | 118.515 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5250 | 118.525 | ACC-U | TWR | TWR | TWR, APP | TWR | TWR |
| 118.5250 | 118.530 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5333 | 118.535 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5417 | 118.540 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5500 | 118.550 | ACC-U | TWR | TWR | TWR, APP | TWR | TWR |
| 118.5500 | 118.555 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5583 | 118.560 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5667 | 118.565 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5750 | 118.575 | ACC-U | TWR | TWR | TWR, APP | TWR | TWR |
| 118.5750 | 118.580 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5833 | 118.585 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.5917 | 118.590 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6000 | 118.600 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.6000 | 118.605 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6083 | 118.610 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6167 | 118.615 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6250 | 118.625 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.6250 | 118.630 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6333 | 118.635 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6417 | 118.640 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6500 | 118.650 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.6500 | 118.655 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6583 | 118.660 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6667 | 118.665 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6750 | 118.675 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.6750 | 118.680 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6833 | 118.685 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.6917 | 118.690 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7000 | 118.700 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.7000 | 118.705 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7083 | 118.710 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7167 | 118.715 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7250 | 118.725 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.7250 | 118.730 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7333 | 118.735 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7417 | 118.740 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7500 | 118.750 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.7500 | 118.755 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7583 | 118.760 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7667 | 118.765 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7750 | 118.775 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.7750 | 118.780 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7833 | 118.785 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.7917 | 118.790 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8000 | 118.800 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.8000 | 118.805 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8083 | 118.810 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8167 | 118.815 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8250 | 118.825 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.8250 | 118.830 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8333 | 118.835 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8417 | 118.840 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8500 | 118.850 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.8500 | 118.855 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8583 | 118.860 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8667 | 118.865 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8750 | 118.875 | TWR | TWR | TWR | TWR, APP | TWR | TWR |
| 118.8750 | 118.880 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8833 | 118.885 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.8917 | 118.890 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9000 | 118.900 | TWR | ACC-L, ACC-U | TWR | TWR, APP | ACC-L, ACC-U | TWR |
| 118.9000 | 118.905 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9083 | 118.910 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9167 | 118.915 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9250 | 118.925 | TWR | ACC-L, ACC-U | TWR | TWR, APP | ACC-L, ACC-U | TWR |
| 118.9250 | 118.930 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9333 | 118.935 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9417 | 118.940 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9500 | 118.950 | TWR | ACC-L, ACC-U | Not allotted | TWR, APP | ACC-L, ACC-U | Not allotted |
| 118.9500 | 118.955 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9583 | 118.960 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9667 | 118.965 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9750 | 118.975 | TWR | ACC-L, ACC-U | Not allotted | TWR, APP | ACC-L, ACC-U | Not allotted |
| 118.9750 | 118.980 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9833 | 118.985 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 118.9917 | 118.990 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0000 | 119.000 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.0000 | 119.005 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0083 | 119.010 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0167 | 119.015 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0250 | 119.025 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.0250 | 119.030 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0333 | 119.035 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0417 | 119.040 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0500 | 119.050 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.0500 | 119.055 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0583 | 119.060 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0667 | 119.065 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0750 | 119.075 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.0750 | 119.080 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0833 | 119.085 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.0917 | 119.090 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1000 | 119.100 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.1000 | 119.105 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1083 | 119.110 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1167 | 119.115 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1250 | 119.125 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.1250 | 119.130 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1333 | 119.135 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1417 | 119.140 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1500 | 119.150 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.1500 | 119.155 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1583 | 119.160 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1667 | 119.165 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1750 | 119.175 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.1750 | 119.180 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1833 | 119.185 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.1917 | 119.190 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2000 | 119.200 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.2000 | 119.205 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2083 | 119.210 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2167 | 119.215 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2250 | 119.225 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.2250 | 119.230 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2333 | 119.235 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2417 | 119.240 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2500 | 119.250 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.2500 | 119.255 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2583 | 119.260 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2667 | 119.265 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2750 | 119.275 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.2750 | 119.280 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2833 | 119.285 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.2917 | 119.290 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3000 | 119.300 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 119.3000 | 119.305 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3083 | 119.310 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3167 | 119.315 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3250 | 119.325 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 119.3250 | 119.330 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3333 | 119.335 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3417 | 119.340 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3500 | 119.350 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 119.3500 | 119.355 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3583 | 119.360 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3667 | 119.365 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3750 | 119.375 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 119.3750 | 119.380 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3833 | 119.385 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.3917 | 119.390 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4000 | 119.400 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.4000 | 119.405 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4083 | 119.410 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4167 | 119.415 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4250 | 119.425 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.4250 | 119.430 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4333 | 119.435 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4417 | 119.440 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4500 | 119.450 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.4500 | 119.455 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4583 | 119.460 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4667 | 119.465 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4750 | 119.475 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.4750 | 119.480 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4833 | 119.485 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.4917 | 119.490 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5000 | 119.505 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5000 | 119.500 | APP-PAR | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.5083 | 119.510 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5167 | 119.515 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5250 | 119.525 | APP-PAR | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.5250 | 119.530 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5333 | 119.535 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5417 | 119.540 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5500 | 119.550 | APP-PAR | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.5500 | 119.555 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5583 | 119.560 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5667 | 119.565 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5750 | 119.575 | APP-PAR | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.5750 | 119.580 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5833 | 119.585 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.5917 | 119.590 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6000 | 119.600 | APP-L | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.6000 | 119.605 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6083 | 119.610 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6167 | 119.615 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6250 | 119.625 | APP-L | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.6250 | 119.630 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6333 | 119.635 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6417 | 119.640 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6500 | 119.650 | APP-L | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.6500 | 119.655 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6583 | 119.660 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6667 | 119.665 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6750 | 119.675 | APP-L | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.6750 | 119.680 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6833 | 119.685 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.6917 | 119.690 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.7000 | 119.700 | APP-L | APP-L, APP-I | APP | RGA (TWR, APP) | APP-L, APP-I | APP |
| 119.7000 | 119.705 | Not used | Not used | Not used | RGA (TWR, APP) | Not used | Not used |
| 119.7083 | 119.710 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.7167 | 119.715 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.7250 | 119.725 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.7250 | 119.730 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.7333 | 119.735 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.7417 | 119.740 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.7500 | 119.750 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.7500 | 119.755 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.7583 | 119.760 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.7667 | 119.765 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.7750 | 119.775 | APP-L | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 119.7750 | 119.780 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.7833 | 119.785 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.7917 | 119.790 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8000 | 119.800 | APP-L | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.8000 | 119.805 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8083 | 119.810 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8167 | 119.815 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8250 | 119.825 | APP-L | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.8250 | 119.830 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8333 | 119.835 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8417 | 119.840 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8500 | 119.850 | APP-L | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.8500 | 119.855 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8583 | 119.860 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8667 | 119.865 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8750 | 119.875 | APP-L | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.8750 | 119.880 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8833 | 119.885 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.8917 | 119.890 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9000 | 119.900 | APP-PAR | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.9000 | 119.905 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9083 | 119.910 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9167 | 119.915 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9250 | 119.930 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9250 | 119.925 | APP-PAR | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.9333 | 119.935 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9417 | 119.940 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9500 | 119.950 | APP-PAR | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.9500 | 119.955 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9583 | 119.960 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9667 | 119.965 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9750 | 119.975 | APP-PAR | APP-PAR | APP | TWR, APP | APP-PAR | APP |
| 119.9750 | 119.980 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9833 | 119.985 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 119.9917 | 119.990 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0000 | 120.000 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.0000 | 120.005 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0083 | 120.010 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0167 | 120.015 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0250 | 120.025 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.0250 | 120.030 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0333 | 120.035 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0417 | 120.040 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0500 | 120.055 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0500 | 120.050 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.0583 | 120.060 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0667 | 120.065 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0750 | 120.075 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.0750 | 120.080 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0833 | 120.085 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.0917 | 120.090 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1000 | 120.100 | APP-PAR | FIS-L, FIS-U | APP | TWR, APP | FIS-L, FIS-U | APP |
| 120.1000 | 120.105 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1083 | 120.110 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1167 | 120.115 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1250 | 120.125 | APP-PAR | FIS-L, FIS-U | APP | TWR, APP | FIS-L, FIS-U | APP |
| 120.1250 | 120.130 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1333 | 120.135 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1417 | 120.140 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1500 | 120.150 | APP-PAR | FIS-L, FIS-U | APP | TWR, APP | FIS-L, FIS-U | APP |
| 120.1500 | 120.155 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1583 | 120.160 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1667 | 120.165 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1750 | 120.175 | APP-PAR | FIS-L, FIS-U | APP | TWR, APP | FIS-L, FIS-U | APP |
| 120.1750 | 120.180 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1833 | 120.185 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.1917 | 120.190 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2000 | 120.200 | Not allotted | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.2000 | 120.205 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2083 | 120.210 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2167 | 120.215 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2250 | 120.225 | Not allotted | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.2250 | 120.230 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2333 | 120.235 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2417 | 120.240 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2500 | 120.250 | Not allotted | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.2500 | 120.255 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2583 | 120.260 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2667 | 120.265 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2750 | 120.275 | Not allotted | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.2750 | 120.280 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2833 | 120.285 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.2917 | 120.290 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3000 | 120.300 | APP-I | APP-U | APP | TWR, APP | APP-U | APP |
| 120.3000 | 120.305 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3083 | 120.310 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3167 | 120.315 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3250 | 120.325 | APP-I | APP-U | APP | TWR, APP | APP-U | APP |
| 120.3250 | 120.330 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3333 | 120.335 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3417 | 120.340 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3500 | 120.350 | APP-I | APP-U | APP | TWR, APP | APP-U | APP |
| 120.3500 | 120.355 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3583 | 120.360 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3667 | 120.365 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3750 | 120.375 | APP-I | APP-U | APP | TWR, APP | APP-U | APP |
| 120.3750 | 120.380 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3833 | 120.385 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.3917 | 120.390 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4000 | 120.400 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.4000 | 120.405 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4083 | 120.410 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4167 | 120.415 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4250 | 120.425 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.4250 | 120.430 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4333 | 120.435 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4417 | 120.440 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4500 | 120.450 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.4500 | 120.455 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4583 | 120.460 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4667 | 120.465 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4750 | 120.475 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.4750 | 120.480 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4833 | 120.485 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.4917 | 120.490 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5000 | 120.500 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.5000 | 120.505 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5083 | 120.510 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5167 | 120.515 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5250 | 120.525 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.5250 | 120.530 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5333 | 120.535 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5417 | 120.540 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5500 | 120.550 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.5500 | 120.555 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5583 | 120.560 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5667 | 120.565 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5750 | 120.575 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.5750 | 120.580 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5833 | 120.585 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.5917 | 120.590 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6000 | 120.600 | ACC-U | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.6000 | 120.605 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6083 | 120.610 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6167 | 120.615 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6250 | 120.625 | ACC-U | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.6250 | 120.630 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6333 | 120.635 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6417 | 120.640 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6500 | 120.650 | ACC-U | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.6500 | 120.655 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6583 | 120.660 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6667 | 120.665 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6750 | 120.675 | ACC-U | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.6750 | 120.680 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6833 | 120.685 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.6917 | 120.690 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7000 | 120.700 | APP-I | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.7000 | 120.705 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7083 | 120.710 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7167 | 120.715 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7250 | 120.725 | APP-I | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.7250 | 120.730 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7333 | 120.735 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7417 | 120.740 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7500 | 120.750 | APP-I | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.7500 | 120.755 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7583 | 120.760 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7667 | 120.765 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7750 | 120.775 | APP-I | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.7750 | 120.780 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7833 | 120.785 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.7917 | 120.790 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8000 | 120.800 | TWR | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.8000 | 120.805 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8083 | 120.810 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8167 | 120.815 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8250 | 120.825 | TWR | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.8250 | 120.830 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8333 | 120.835 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8417 | 120.840 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8500 | 120.850 | TWR | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.8500 | 120.855 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8583 | 120.860 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8667 | 120.865 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8750 | 120.875 | TWR | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 120.8750 | 120.880 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8833 | 120.885 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.8917 | 120.890 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9000 | 120.900 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.9000 | 120.905 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9083 | 120.910 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9167 | 120.915 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9250 | 120.925 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.9250 | 120.930 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9333 | 120.935 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9417 | 120.940 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9500 | 120.950 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.9500 | 120.955 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9583 | 120.960 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9667 | 120.965 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9750 | 120.980 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9750 | 120.975 | ACC-U | ACC-L, ACC-U | APP | TWR, APP | ACC-L, ACC-U | APP |
| 120.9833 | 120.985 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 120.9917 | 120.990 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0000 | 121.000 | Not allotted | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.0000 | 121.005 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0083 | 121.010 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0167 | 121.015 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0250 | 121.025 | Not allotted | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.0250 | 121.030 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0333 | 121.035 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0417 | 121.040 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0500 | 121.050 | Not allotted | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.0500 | 121.055 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0583 | 121.060 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0667 | 121.065 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0750 | 121.075 | Not allotted | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.0750 | 121.080 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0833 | 121.085 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.0917 | 121.090 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1000 | 121.100 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.1000 | 121.105 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1083 | 121.110 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1167 | 121.115 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1250 | 121.125 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.1250 | 121.130 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1333 | 121.135 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1417 | 121.140 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1500 | 121.150 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.1500 | 121.155 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1583 | 121.160 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1667 | 121.165 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1750 | 121.175 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.1750 | 121.180 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1833 | 121.185 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.1917 | 121.190 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2000 | 121.200 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.2000 | 121.205 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2083 | 121.210 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2167 | 121.215 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2250 | 121.225 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.2250 | 121.230 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2333 | 121.235 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2417 | 121.240 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2500 | 121.250 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.2500 | 121.255 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2583 | 121.260 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2667 | 121.265 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2750 | 121.275 | APP-I | APP-L, APP-I | APP | TWR, APP | APP-L, APP-I | APP |
| 121.2750 | 121.280 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2833 | 121.285 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.2917 | 121.290 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3000 | 121.300 | APP-I | APP-U | APP | TWR, APP | APP-U | APP |
| 121.3000 | 121.305 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3083 | 121.310 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3167 | 121.315 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3250 | 121.325 | APP-I | APP-U | APP | TWR, APP | APP-U | APP |
| 121.3250 | 121.330 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3333 | 121.335 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3417 | 121.340 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3500 | 121.350 | APP-I | APP-U | APP | TWR, APP | APP-U | APP |
| 121.3500 | 121.355 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3583 | 121.360 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3667 | 121.365 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3750 | 121.375 | APP-I | APP-U | APP | TWR, APP | APP-U | APP |
| 121.3750 | 121.380 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3833 | 121.385 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.3917 | 121.390 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
|  |  |  |  |  |  |  |  |
| 121.4000 | 121.400 | APP-I | APP-L, APP-I | Not allotted | TWR, APP | APP-L, APP-I | Not allotted |
| 121.4000 | 121.405 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.4083 | 121.410 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.4167 | 121.415 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.4250 | 121.425 | APP-I | APP-L, APP-I | Not allotted | TWR, APP | APP-L, APP-I | Not allotted |
| 121.4250 | 121.430 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.4333 | 121.435 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.4417 | 121.440 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.4500 | 121.450 | APP-I | APP-L, APP-I | Not allotted | TWR, APP | APP-L, APP-I | Not allotted |
| 121.4500 | 121.455 | Not used | Not used | Not used | TWR, APP | Not used | Not used |
| 121.4583 | 121.460 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.4667 | 121.465 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.4750 | 121.475 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.4750 | 121.480 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.4833 | 121.485 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.4917 | 121.490 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.5000 | 121.500 | Emerg. | Emerg. | Emerg. | Emerg. | Emerg. | Emerg. |
| 121.5000 | 121.505 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.5083 | 121.510 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.5167 | 121.515 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.5250 | 121.525 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.5250 | 121.530 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.5333 | 121.535 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.5417 | 121.540 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 121.5500 | 121.550 | AS | AS | AS | AS | AS | AS |
| 121.5500 | 121.555 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.5583 | 121.560 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.5667 | 121.565 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.5750 | 121.575 | AS | AS | AS | AS | AS | AS |
| 121.5750 | 121.580 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.5833 | 121.585 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.5917 | 121.590 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6000 | 121.600 | AS | AS | AS | AS | AS | AS |
| 121.6000 | 121.605 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6083 | 121.610 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6167 | 121.615 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6250 | 121.630 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6250 | 121.625 | AS | AS | AS | AS | AS | AS |
| 121.6333 | 121.635 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6417 | 121.640 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6500 | 121.650 | AS | AS | AS | AS | AS | AS |
| 121.6500 | 121.655 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6583 | 121.660 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6667 | 121.665 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6750 | 121.675 | AS | AS | AS | AS | AS | AS |
| 121.6750 | 121.680 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6833 | 121.685 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.6917 | 121.690 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7000 | 121.700 | AS | AS | AS | AS | AS | AS |
| 121.7000 | 121.705 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7083 | 121.710 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7167 | 121.715 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7250 | 121.725 | AS | AS | AS | AS | AS | AS |
| 121.7250 | 121.730 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7333 | 121.735 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7417 | 121.740 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7500 | 121.750 | AS | AS | AS | AS | AS | AS |
| 121.7500 | 121.755 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7583 | 121.760 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7667 | 121.765 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7750 | 121.775 | AS | AS | AS | AS | AS | AS |
| 121.7750 | 121.780 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7833 | 121.785 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.7917 | 121.790 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8000 | 121.800 | AS | AS | AS | AS | AS | AS |
| 121.8000 | 121.805 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8083 | 121.810 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8167 | 121.815 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8250 | 121.825 | AS | AS | AS | AS | AS | AS |
| 121.8250 | 121.830 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8333 | 121.835 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8417 | 121.840 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8500 | 121.850 | AS | AS | AS | AS | AS | AS |
| 121.8500 | 121.855 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8583 | 121.860 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8667 | 121.865 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8750 | 121.875 | AS | AS | AS | AS | AS | AS |
| 121.8750 | 121.880 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8833 | 121.885 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.8917 | 121.890 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9000 | 121.900 | AS | AS | AS | AS | AS | AS |
| 121.9000 | 121.905 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9083 | 121.910 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9167 | 121.915 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9250 | 121.925 | AS | AS | AS | AS | AS | AS |
| 121.9250 | 121.930 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9333 | 121.935 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9417 | 121.940 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9500 | 121.950 | AS | AS | AS | AS | AS | AS |
| 121.9500 | 121.955 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9583 | 121.960 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9667 | 121.965 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9750 | 121.975 | AS | AS | AS | AS | AS | AS |
| 121.9750 | 121.980 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9833 | 121.985 | Not used | Not used | Not used | AS | Not used | Not used |
| 121.9917 | 121.990 | Not used | Not used | Not used | AS | Not used | Not used |
| 122.0000 | 122.000 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.0000 | 122.005 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.0083 | 122.010 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.0167 | 122.015 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.0250 | 122.025 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.0250 | 122.030 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.0333 | 122.035 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.0417 | 122.040 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.0500 | 122.050 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.0500 | 122.055 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.0583 | 122.060 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.0667 | 122.065 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.0750 | 122.075 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.0750 | 122.080 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.0833 | 122.085 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.0917 | 122.090 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.1000 | 122.100 | Not allotted | Not allotted | Not allotted | RGA TWR, APP | Not allotted | Not allotted |
| 122.1000 | 122.105 | Not used | Not used | Not used | RGA TWR, APP | Not used | Not used |
| 122.1083 | 122.110 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.1167 | 122.115 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.1250 | 122.125 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.1250 | 122.130 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.1333 | 122.135 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.1417 | 122.140 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.1500 | 122.150 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.1500 | 122.155 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.1583 | 122.160 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.1667 | 122.165 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.1750 | 122.175 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.1750 | 122.180 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.1833 | 122.185 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.1917 | 122.190 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2000 | 122.200 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.2000 | 122.205 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2083 | 122.210 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2167 | 122.215 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2250 | 122.225 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.2250 | 122.230 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2333 | 122.235 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2417 | 122.240 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2500 | 122.250 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.2500 | 122.255 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2583 | 122.260 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2667 | 122.265 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2750 | 122.275 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.2750 | 122.280 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2833 | 122.285 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.2917 | 122.290 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3000 | 122.300 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.3000 | 122.305 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3083 | 122.310 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3167 | 122.315 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3250 | 122.325 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.3250 | 122.330 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3333 | 122.335 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3417 | 122.340 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3500 | 122.350 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.3500 | 122.355 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3583 | 122.360 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3667 | 122.365 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3750 | 122.375 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.3750 | 122.380 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3833 | 122.385 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.3917 | 122.390 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4000 | 122.400 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.4000 | 122.405 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4083 | 122.410 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4167 | 122.415 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4250 | 122.425 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.4250 | 122.430 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4333 | 122.435 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4417 | 122.440 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4500 | 122.450 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.4500 | 122.455 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4583 | 122.460 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4667 | 122.465 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4750 | 122.475 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.4750 | 122.480 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4833 | 122.485 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.4917 | 122.490 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.5000 | 122.500 | Not allotted | Not allotted | Not allotted | RLA | Not allotted | Not allotted |
| 122.5000 | 122.505 | Not used | Not used | Not used | RLA | Not used | Not used |
| 122.5083 | 122.510 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.5167 | 122.515 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.5250 | 122.525 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.5250 | 122.530 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.5333 | 122.535 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.5417 | 122.540 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.5500 | 122.550 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.5500 | 122.555 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.5583 | 122.560 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.5667 | 122.565 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.5750 | 122.575 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.5750 | 122.580 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.5833 | 122.585 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.5917 | 122.590 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6000 | 122.600 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.6000 | 122.605 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6083 | 122.610 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6167 | 122.615 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6250 | 122.625 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.6250 | 122.630 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6333 | 122.635 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6417 | 122.640 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6500 | 122.650 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.6500 | 122.655 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6583 | 122.660 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6667 | 122.665 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6750 | 122.675 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.6750 | 122.680 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6833 | 122.685 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.6917 | 122.690 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7000 | 122.700 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.7000 | 122.705 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7083 | 122.710 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7167 | 122.715 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7250 | 122.725 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.7250 | 122.730 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7333 | 122.735 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7417 | 122.740 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7500 | 122.750 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.7500 | 122.755 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7583 | 122.760 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7667 | 122.765 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7750 | 122.775 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.7750 | 122.780 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7833 | 122.785 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.7917 | 122.790 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8000 | 122.800 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.8000 | 122.805 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8083 | 122.810 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8167 | 122.815 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8250 | 122.825 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.8250 | 122.830 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8333 | 122.835 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8417 | 122.840 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8500 | 122.850 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.8500 | 122.855 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8583 | 122.860 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8667 | 122.865 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8750 | 122.875 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.8750 | 122.880 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8833 | 122.885 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.8917 | 122.890 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9000 | 122.900 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.9000 | 122.905 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9083 | 122.910 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9167 | 122.915 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9250 | 122.925 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.9250 | 122.930 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9333 | 122.935 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9417 | 122.940 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9500 | 122.950 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.9500 | 122.955 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9583 | 122.960 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9667 | 122.965 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9750 | 122.975 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 122.9750 | 122.980 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9833 | 122.985 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 122.9917 | 122.990 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.0000 | 123.000 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.0000 | 123.005 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.0083 | 123.010 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.0167 | 123.015 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.0250 | 123.025 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.0250 | 123.030 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.0333 | 123.035 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.0417 | 123.040 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.0500 | 123.050 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.0500 | 123.055 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.0583 | 123.060 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.0667 | 123.065 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.0750 | 123.075 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.0750 | 123.080 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.0833 | 123.085 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.0917 | 123.090 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.1000 | 123.100 | SAR | SAR | SAR | SAR | SAR | SAR |
| 123.1000 | 123.105 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.1083 | 123.110 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.1167 | 123.115 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.1250 | 123.125 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.1250 | 123.130 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.1333 | 123.135 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.1417 | 123.140 | Blocked | Blocked | Blocked | Blocked | Blocked | Blocked |
| 123.1500 | 123.150 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.1500 | 123.155 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.1583 | 123.160 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.1667 | 123.165 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.1750 | 123.175 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.1750 | 123.180 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.1833 | 123.185 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.1917 | 123.190 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2000 | 123.200 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.2000 | 123.205 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2083 | 123.210 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2167 | 123.215 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2250 | 123.225 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.2250 | 123.230 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2333 | 123.235 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2417 | 123.240 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2500 | 123.255 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2500 | 123.250 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.2583 | 123.260 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2667 | 123.265 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2750 | 123.275 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.2750 | 123.280 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2833 | 123.285 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.2917 | 123.290 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3000 | 123.300 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.3000 | 123.305 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3083 | 123.310 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3167 | 123.315 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3250 | 123.325 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.3250 | 123.330 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3333 | 123.335 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3417 | 123.340 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3500 | 123.350 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.3500 | 123.355 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3583 | 123.360 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3667 | 123.365 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3750 | 123.375 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.3750 | 123.380 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3833 | 123.385 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.3917 | 123.390 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4000 | 123.400 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.4000 | 123.405 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4083 | 123.410 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4167 | 123.415 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4250 | 123.425 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.4250 | 123.430 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4333 | 123.435 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4417 | 123.440 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4500 | 123.450 | Air-Air | Air-Air | Air-Air | Not allotted | Air-Air | Air-Air |
| 123.4500 | 123.455 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4583 | 123.460 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4667 | 123.465 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4750 | 123.475 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.4750 | 123.480 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4833 | 123.485 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.4917 | 123.490 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5000 | 123.500 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.5000 | 123.505 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5083 | 123.510 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5167 | 123.515 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5250 | 123.525 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.5250 | 123.530 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5333 | 123.535 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5417 | 123.540 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5500 | 123.550 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.5500 | 123.555 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5583 | 123.560 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5667 | 123.565 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5750 | 123.575 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.5750 | 123.580 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5833 | 123.585 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.5917 | 123.590 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6000 | 123.600 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.6000 | 123.605 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6083 | 123.610 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6167 | 123.615 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6250 | 123.625 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.6250 | 123.630 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6333 | 123.635 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6417 | 123.640 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6500 | 123.650 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.6500 | 123.655 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6583 | 123.660 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6667 | 123.665 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6750 | 123.675 | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted | Not allotted |
| 123.6750 | 123.680 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6833 | 123.685 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.6917 | 123.690 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 123.7000 | 123.700 | APP-I | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 123.7000 | 123.705 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.7083 | 123.710 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.7167 | 123.715 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.7250 | 123.725 | APP-I | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 123.7250 | 123.730 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.7333 | 123.735 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.7417 | 123.740 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.7500 | 123.750 | APP-I | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 123.7500 | 123.755 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.7583 | 123.760 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.7667 | 123.765 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.7750 | 123.775 | APP-I | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 123.7750 | 123.780 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.7833 | 123.785 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.7917 | 123.790 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8000 | 123.800 | ACC-L | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 123.8000 | 123.805 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8083 | 123.810 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8167 | 123.815 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8250 | 123.825 | ACC-L | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 123.8250 | 123.830 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8333 | 123.835 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8417 | 123.840 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8500 | 123.850 | ACC-L | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 123.8500 | 123.855 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8583 | 123.860 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8667 | 123.865 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8750 | 123.875 | ACC-L | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 123.8750 | 123.880 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8833 | 123.885 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.8917 | 123.890 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9000 | 123.900 | APP-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 123.9000 | 123.905 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9083 | 123.910 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9167 | 123.915 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9250 | 123.925 | APP-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 123.9250 | 123.930 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9333 | 123.935 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9417 | 123.940 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9500 | 123.950 | APP-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 123.9500 | 123.955 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9583 | 123.960 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9667 | 123.965 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9750 | 123.975 | APP-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 123.9750 | 123.980 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9833 | 123.985 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 123.9917 | 123.990 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0000 | 124.000 | APP-I | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 124.0000 | 124.005 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0083 | 124.010 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0167 | 124.015 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0250 | 124.025 | APP-I | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 124.0250 | 124.030 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0333 | 124.035 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0417 | 124.040 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0500 | 124.050 | APP-I | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 124.0500 | 124.055 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0583 | 124.060 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0667 | 124.065 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0750 | 124.075 | APP-I | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 124.0750 | 124.080 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0833 | 124.085 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.0917 | 124.090 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1000 | 124.100 | Not allotted | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 124.1000 | 124.105 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1083 | 124.110 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1167 | 124.115 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1250 | 124.125 | Not allotted | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 124.1250 | 124.130 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1333 | 124.135 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1417 | 124.140 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1500 | 124.150 | Not allotted | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 124.1500 | 124.155 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1583 | 124.160 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1667 | 124.165 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1750 | 124.175 | Not allotted | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 124.1750 | 124.180 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1833 | 124.185 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.1917 | 124.190 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2000 | 124.200 | FIS-L | APP-U | ACC | APP, ACC-L | Not allotted | ACC |
| 124.2000 | 124.205 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2083 | 124.210 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2167 | 124.215 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2250 | 124.225 | FIS-L | APP-U | ACC | APP, ACC-L | Not allotted | ACC |
| 124.2250 | 124.230 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2333 | 124.235 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2417 | 124.240 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2500 | 124.250 | FIS-L | APP-U | ACC | APP, ACC-L | Not allotted | ACC |
| 124.2500 | 124.255 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2583 | 124.260 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2667 | 124.265 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2750 | 124.275 | FIS-L | APP-U | ACC | APP, ACC-L | Not allotted | ACC |
| 124.2750 | 124.280 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2833 | 124.285 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.2917 | 124.290 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3000 | 124.300 | APP-I | TWR | ACC | APP, ACC-L | TWR | ACC |
| 124.3000 | 124.305 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3083 | 124.310 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3167 | 124.315 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3250 | 124.325 | APP-I | TWR | ACC | APP, ACC-L | TWR | ACC |
| 124.3250 | 124.330 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3333 | 124.335 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3417 | 124.340 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3500 | 124.350 | APP-I | TWR | ACC | APP, ACC-L | TWR | ACC |
| 124.3500 | 124.355 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3583 | 124.360 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3667 | 124.365 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3750 | 124.375 | APP-I | TWR | ACC | APP, ACC-L | TWR | ACC |
| 124.3750 | 124.380 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3833 | 124.385 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.3917 | 124.390 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4000 | 124.400 | APP-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.4000 | 124.405 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4083 | 124.410 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4167 | 124.415 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4250 | 124.425 | APP-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.4250 | 124.430 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4333 | 124.435 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4417 | 124.440 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4500 | 124.450 | APP-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.4500 | 124.455 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4583 | 124.460 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4667 | 124.465 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4750 | 124.475 | APP-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.4750 | 124.480 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4833 | 124.485 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.4917 | 124.490 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5000 | 124.500 | APP-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 124.5000 | 124.505 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5083 | 124.510 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5167 | 124.515 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5250 | 124.525 | APP-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 124.5250 | 124.530 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5333 | 124.535 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5417 | 124.540 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5500 | 124.550 | APP-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 124.5500 | 124.555 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5583 | 124.560 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5667 | 124.565 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5750 | 124.575 | APP-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 124.5750 | 124.580 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5833 | 124.585 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.5917 | 124.590 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6000 | 124.600 | ACC-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.6000 | 124.605 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6083 | 124.610 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6167 | 124.615 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6250 | 124.625 | ACC-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.6250 | 124.630 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6333 | 124.635 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6417 | 124.640 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6500 | 124.650 | ACC-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.6500 | 124.655 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6583 | 124.660 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6667 | 124.665 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6750 | 124.675 | ACC-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.6750 | 124.680 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6833 | 124.685 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.6917 | 124.690 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7000 | 124.700 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 124.7000 | 124.705 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7083 | 124.710 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7167 | 124.715 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7250 | 124.725 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 124.7250 | 124.730 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7333 | 124.735 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7417 | 124.740 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7500 | 124.750 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 124.7500 | 124.755 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7583 | 124.760 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7667 | 124.765 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7750 | 124.775 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 124.7750 | 124.780 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7833 | 124.785 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.7917 | 124.790 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8000 | 124.800 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.8000 | 124.805 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8083 | 124.810 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8167 | 124.815 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8250 | 124.825 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.8250 | 124.830 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8333 | 124.835 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8417 | 124.840 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8500 | 124.850 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.8500 | 124.855 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8583 | 124.860 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8667 | 124.865 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8750 | 124.875 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 124.8750 | 124.880 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8833 | 124.885 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.8917 | 124.890 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9000 | 124.900 | APP-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 124.9000 | 124.905 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9083 | 124.910 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9167 | 124.915 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9250 | 124.925 | APP-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 124.9250 | 124.930 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9333 | 124.935 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9417 | 124.940 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9500 | 124.950 | APP-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 124.9500 | 124.955 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9583 | 124.960 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9667 | 124.965 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9750 | 124.975 | APP-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 124.9750 | 124.980 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9833 | 124.985 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 124.9917 | 124.990 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0000 | 125.000 | Not allotted | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.0000 | 125.005 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0083 | 125.010 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0167 | 125.015 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0250 | 125.025 | Not allotted | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.0250 | 125.030 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0333 | 125.035 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0417 | 125.040 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0500 | 125.050 | Not allotted | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.0500 | 125.055 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0583 | 125.060 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0667 | 125.065 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0750 | 125.075 | Not allotted | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.0750 | 125.080 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0833 | 125.085 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.0917 | 125.090 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1000 | 125.100 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 125.1000 | 125.105 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1083 | 125.110 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1167 | 125.115 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1250 | 125.125 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 125.1250 | 125.130 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1333 | 125.135 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1417 | 125.140 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1500 | 125.150 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 125.1500 | 125.155 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1583 | 125.160 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1667 | 125.165 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1750 | 125.175 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 125.1750 | 125.180 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1833 | 125.185 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.1917 | 125.190 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2000 | 125.200 | FIS-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.2000 | 125.205 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2083 | 125.210 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2167 | 125.215 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2250 | 125.225 | FIS-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.2250 | 125.230 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2333 | 125.235 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2417 | 125.240 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2500 | 125.250 | FIS-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.2500 | 125.255 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2583 | 125.260 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2667 | 125.265 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2750 | 125.275 | FIS-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.2750 | 125.280 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2833 | 125.285 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.2917 | 125.290 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3000 | 125.300 | APP-I | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.3000 | 125.305 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3083 | 125.310 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3167 | 125.315 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3250 | 125.325 | APP-I | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.3250 | 125.330 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3333 | 125.335 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3417 | 125.340 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3500 | 125.350 | APP-I | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.3500 | 125.355 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3583 | 125.360 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3667 | 125.365 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3750 | 125.375 | APP-I | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.3750 | 125.380 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3833 | 125.385 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.3917 | 125.390 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4000 | 125.400 | ACC-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.4000 | 125.405 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4083 | 125.410 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4167 | 125.415 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4250 | 125.425 | ACC-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.4250 | 125.430 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4333 | 125.435 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4417 | 125.440 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4500 | 125.450 | ACC-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.4500 | 125.455 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4583 | 125.460 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4667 | 125.465 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4750 | 125.475 | ACC-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.4750 | 125.480 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4833 | 125.485 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.4917 | 125.490 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5000 | 125.500 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 125.5000 | 125.505 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5083 | 125.510 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5167 | 125.515 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5250 | 125.525 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 125.5250 | 125.530 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5333 | 125.535 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5417 | 125.540 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5500 | 125.550 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 125.5500 | 125.555 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5583 | 125.560 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5667 | 125.565 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5750 | 125.575 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 125.5750 | 125.580 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5833 | 125.585 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.5917 | 125.590 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6000 | 125.600 | ACC-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.6000 | 125.605 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6083 | 125.610 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6167 | 125.615 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6250 | 125.625 | ACC-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.6250 | 125.630 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6333 | 125.635 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6417 | 125.640 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6500 | 125.650 | ACC-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.6500 | 125.655 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6583 | 125.660 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6667 | 125.665 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6750 | 125.675 | ACC-U | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.6750 | 125.680 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6833 | 125.685 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.6917 | 125.690 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7000 | 125.700 | APP-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.7000 | 125.705 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7083 | 125.710 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7167 | 125.715 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7250 | 125.725 | APP-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.7250 | 125.730 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7333 | 125.735 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7417 | 125.740 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7500 | 125.750 | APP-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.7500 | 125.755 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7583 | 125.760 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7667 | 125.765 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7750 | 125.775 | APP-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.7750 | 125.780 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7833 | 125.785 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.7917 | 125.790 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8000 | 125.800 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.8000 | 125.805 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8083 | 125.810 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8167 | 125.815 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8250 | 125.825 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.8250 | 125.830 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8333 | 125.835 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8417 | 125.840 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8500 | 125.850 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.8500 | 125.855 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8583 | 125.860 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8667 | 125.865 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8750 | 125.875 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 125.8750 | 125.880 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8833 | 125.885 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.8917 | 125.890 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9000 | 125.900 | ACC-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.9000 | 125.905 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9083 | 125.910 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9167 | 125.915 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9250 | 125.925 | ACC-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.9250 | 125.930 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9333 | 125.935 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9417 | 125.940 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9500 | 125.950 | ACC-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.9500 | 125.955 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9583 | 125.960 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9667 | 125.965 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9750 | 125.975 | ACC-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 125.9750 | 125.980 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9833 | 125.985 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 125.9917 | 125.990 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0000 | 126.000 | APP-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 126.0000 | 126.005 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0083 | 126.010 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0167 | 126.015 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0250 | 126.025 | APP-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 126.0250 | 126.030 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0333 | 126.035 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0417 | 126.040 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0500 | 126.050 | APP-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 126.0500 | 126.055 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0583 | 126.060 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0667 | 126.065 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0750 | 126.075 | APP-L | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 126.0750 | 126.080 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0833 | 126.085 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.0917 | 126.090 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1000 | 126.100 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 126.1000 | 126.105 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1083 | 126.110 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1167 | 126.115 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1250 | 126.125 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 126.1250 | 126.130 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1333 | 126.135 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1417 | 126.140 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1500 | 126.150 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 126.1500 | 126.155 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1583 | 126.160 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1667 | 126.165 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1750 | 126.175 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 126.1750 | 126.180 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1833 | 126.185 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.1917 | 126.190 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2000 | 126.200 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.2000 | 126.205 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2083 | 126.210 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2167 | 126.215 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2250 | 126.225 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.2250 | 126.230 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2333 | 126.235 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2417 | 126.240 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2500 | 126.250 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.2500 | 126.255 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2583 | 126.260 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2667 | 126.265 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2750 | 126.275 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.2750 | 126.280 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2833 | 126.285 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.2917 | 126.290 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3000 | 126.300 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 126.3000 | 126.305 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3083 | 126.310 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3167 | 126.315 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3250 | 126.325 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 126.3250 | 126.330 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3333 | 126.335 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3417 | 126.340 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3500 | 126.350 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 126.3500 | 126.355 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3583 | 126.360 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3667 | 126.365 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3750 | 126.375 | FIS-U (GPS) | APP-U | ACC | APP, ACC-L | APP-U | ACC |
| 126.3750 | 126.380 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3833 | 126.385 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.3917 | 126.390 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4000 | 126.400 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.4000 | 126.405 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4083 | 126.410 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4167 | 126.415 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4250 | 126.425 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.4250 | 126.430 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4333 | 126.435 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4417 | 126.440 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4500 | 126.450 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.4500 | 126.455 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4583 | 126.460 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4667 | 126.465 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4750 | 126.475 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.4750 | 126.480 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4833 | 126.485 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.4917 | 126.490 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5000 | 126.500 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 126.5000 | 126.505 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5083 | 126.510 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5167 | 126.515 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5250 | 126.525 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 126.5250 | 126.530 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5333 | 126.535 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5417 | 126.540 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5500 | 126.550 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 126.5500 | 126.555 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5583 | 126.560 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5667 | 126.565 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5750 | 126.575 | ACC-U | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 126.5750 | 126.580 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5833 | 126.585 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.5917 | 126.590 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6000 | 126.600 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.6000 | 126.605 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6083 | 126.610 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6167 | 126.615 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6250 | 126.625 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.6250 | 126.630 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6333 | 126.635 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6417 | 126.640 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6500 | 126.650 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.6500 | 126.655 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6583 | 126.660 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6667 | 126.665 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6750 | 126.675 | VOLMET, ATIS | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 126.6750 | 126.680 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6833 | 126.685 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.6917 | 126.690 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7000 | 126.700 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 126.7000 | 126.705 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7083 | 126.710 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7167 | 126.715 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7250 | 126.725 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 126.7250 | 126.730 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7333 | 126.735 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7417 | 126.740 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7500 | 126.750 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 126.7500 | 126.755 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7583 | 126.760 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7667 | 126.765 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7750 | 126.775 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 126.7750 | 126.780 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7833 | 126.785 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.7917 | 126.790 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8000 | 126.800 | VOLMET, ATIS | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 126.8000 | 126.805 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8083 | 126.810 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8167 | 126.815 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8250 | 126.825 | VOLMET, ATIS | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 126.8250 | 126.830 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8333 | 126.835 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8417 | 126.840 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8500 | 126.850 | VOLMET, ATIS | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 126.8500 | 126.855 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8583 | 126.860 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8667 | 126.865 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8750 | 126.875 | VOLMET, ATIS | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 126.8750 | 126.880 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8833 | 126.885 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.8917 | 126.890 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9000 | 126.900 | FIS-U (GPS) | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 126.9000 | 126.905 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9083 | 126.910 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9167 | 126.915 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9250 | 126.925 | FIS-U (GPS) | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 126.9250 | 126.930 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9333 | 126.935 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9417 | 126.940 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9500 | 126.950 | FIS-U (GPS) | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 126.9500 | 126.955 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9583 | 126.960 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9667 | 126.965 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9750 | 126.975 | FIS-U (GPS) | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 126.9750 | 126.980 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9833 | 126.985 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 126.9917 | 126.990 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0000 | 127.000 | VOLMET, ATIS | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.0000 | 127.005 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0083 | 127.010 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0167 | 127.015 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0250 | 127.025 | VOLMET, ATIS | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.0250 | 127.030 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0333 | 127.035 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0417 | 127.040 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0500 | 127.050 | VOLMET, ATIS | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.0500 | 127.055 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0583 | 127.060 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0667 | 127.065 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0750 | 127.075 | VOLMET, ATIS | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.0750 | 127.080 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0833 | 127.085 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.0917 | 127.090 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1000 | 127.100 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 127.1000 | 127.105 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1083 | 127.110 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1167 | 127.115 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1250 | 127.125 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 127.1250 | 127.130 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1333 | 127.135 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1417 | 127.140 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1500 | 127.150 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 127.1500 | 127.155 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1583 | 127.160 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1667 | 127.165 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1750 | 127.175 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 127.1750 | 127.180 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1833 | 127.185 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.1917 | 127.190 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2000 | 127.200 | APP-U | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.2000 | 127.205 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2083 | 127.210 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2167 | 127.215 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2250 | 127.225 | APP-U | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.2250 | 127.230 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2333 | 127.235 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2417 | 127.240 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2500 | 127.250 | APP-U | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.2500 | 127.255 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2583 | 127.260 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2667 | 127.265 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2750 | 127.275 | APP-U | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.2750 | 127.280 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2833 | 127.285 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.2917 | 127.290 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3000 | 127.300 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 127.3000 | 127.305 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3083 | 127.310 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3167 | 127.315 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3250 | 127.325 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 127.3250 | 127.330 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3333 | 127.335 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3417 | 127.340 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3500 | 127.350 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 127.3500 | 127.355 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3583 | 127.360 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3667 | 127.365 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3750 | 127.375 | ACC-U | FIS-L, FIS-U | GPS | APP, ACC-L | FIS-L, FIS-U | GPS |
| 127.3750 | 127.380 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3833 | 127.385 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.3917 | 127.390 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4000 | 127.400 | FIS-U (GPS) | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.4000 | 127.405 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4083 | 127.410 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4167 | 127.415 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4250 | 127.425 | FIS-U (GPS) | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.4250 | 127.430 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4333 | 127.435 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4417 | 127.440 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4500 | 127.450 | FIS-U (GPS) | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.4500 | 127.455 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4583 | 127.460 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4667 | 127.465 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4750 | 127.475 | FIS-U (GPS) | VOLMET, ATIS | GPS | APP, ACC-L | VOLMET, ATIS | GPS |
| 127.4750 | 127.480 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4833 | 127.485 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.4917 | 127.490 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5000 | 127.500 | FIS-L | ACC-L | GPS | APP, ACC-L | ACC-L | GPS |
| 127.5000 | 127.505 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5083 | 127.510 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5167 | 127.515 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5250 | 127.525 | FIS-L | ACC-L | GPS | APP, ACC-L | ACC-L | GPS |
| 127.5250 | 127.530 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5333 | 127.535 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5417 | 127.540 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5500 | 127.550 | FIS-L | ACC-L | GPS | APP, ACC-L | ACC-L | GPS |
| 127.5500 | 127.555 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5583 | 127.560 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5667 | 127.565 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5750 | 127.575 | FIS-L | ACC-L | GPS | APP, ACC-L | ACC-L | GPS |
| 127.5750 | 127.580 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5833 | 127.585 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.5917 | 127.590 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6000 | 127.600 | VOLMET, ATIS | VOLMET, ATIS | VOLMET, ATIS | APP, ACC-L | VOLMET, ATIS | VOLMET, ATIS |
| 127.6000 | 127.605 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6083 | 127.610 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6167 | 127.615 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6250 | 127.625 | VOLMET, ATIS | VOLMET, ATIS | VOLMET, ATIS | APP, ACC-L | VOLMET, ATIS | VOLMET, ATIS |
| 127.6250 | 127.630 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6333 | 127.635 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6417 | 127.640 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6500 | 127.650 | VOLMET, ATIS | VOLMET, ATIS | VOLMET, ATIS | APP, ACC-L | VOLMET, ATIS | VOLMET, ATIS |
| 127.6500 | 127.655 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6583 | 127.660 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6667 | 127.665 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6750 | 127.675 | VOLMET, ATIS | VOLMET, ATIS | VOLMET, ATIS | APP, ACC-L | VOLMET, ATIS | VOLMET, ATIS |
| 127.6750 | 127.680 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6833 | 127.685 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.6917 | 127.690 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7000 | 127.700 | ACC-U | APP-L, APP-I | VOLMET, ATIS | APP, ACC-L | APP-L, APP-I | VOLMET, ATIS |
| 127.7000 | 127.705 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7083 | 127.710 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7167 | 127.715 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7250 | 127.725 | ACC-U | APP-L, APP-I | VOLMET, ATIS | APP, ACC-L | APP-L, APP-I | VOLMET, ATIS |
| 127.7250 | 127.730 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7333 | 127.735 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7417 | 127.740 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7500 | 127.750 | ACC-U | APP-L, APP-I | VOLMET, ATIS | APP, ACC-L | APP-L, APP-I | VOLMET, ATIS |
| 127.7500 | 127.755 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7583 | 127.760 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7667 | 127.765 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7750 | 127.775 | ACC-U | APP-L, APP-I | VOLMET, ATIS | APP, ACC-L | APP-L, APP-I | VOLMET, ATIS |
| 127.7750 | 127.780 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7833 | 127.785 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.7917 | 127.790 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8000 | 127.800 | APP-U | VOLMET, ATIS | VOLMET, ATIS | APP, ACC-L | VOLMET, ATIS | VOLMET, ATIS |
| 127.8000 | 127.805 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8083 | 127.810 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8167 | 127.815 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8250 | 127.825 | APP-U | VOLMET, ATIS | VOLMET, ATIS | APP, ACC-L | VOLMET, ATIS | VOLMET, ATIS |
| 127.8250 | 127.830 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8333 | 127.835 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8417 | 127.840 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8500 | 127.850 | APP-U | VOLMET, ATIS | VOLMET, ATIS | APP, ACC-L | VOLMET, ATIS | VOLMET, ATIS |
| 127.8500 | 127.855 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8583 | 127.860 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8667 | 127.865 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8750 | 127.875 | APP-U | VOLMET, ATIS | VOLMET, ATIS | APP, ACC-L | VOLMET, ATIS | VOLMET, ATIS |
| 127.8750 | 127.880 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8833 | 127.885 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.8917 | 127.890 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9000 | 127.900 | Not allotted | APP-L, APP-I | VOLMET, ATIS | APP, ACC-L | APP-L, APP-I | VOLMET, ATIS |
| 127.9000 | 127.905 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9083 | 127.910 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9167 | 127.915 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9250 | 127.925 | Not allotted | APP-L, APP-I | Not allotted | APP, ACC-L | APP-L, APP-I | Not allotted |
| 127.9250 | 127.930 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9333 | 127.935 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9417 | 127.940 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9500 | 127.950 | Not allotted | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 127.9500 | 127.955 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9583 | 127.960 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9667 | 127.965 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9750 | 127.975 | Not allotted | APP-L, APP-I | ACC | APP, ACC-L | APP-L, APP-I | ACC |
| 127.9750 | 127.980 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9833 | 127.985 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 127.9917 | 127.990 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0000 | 128.000 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.0000 | 128.005 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0083 | 128.010 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0167 | 128.015 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0250 | 128.025 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.0250 | 128.030 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0333 | 128.035 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0417 | 128.040 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0500 | 128.050 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.0500 | 128.055 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0583 | 128.060 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0667 | 128.065 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0750 | 128.075 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.0750 | 128.080 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0833 | 128.085 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.0917 | 128.090 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1000 | 128.100 | ACC-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 128.1000 | 128.105 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1083 | 128.110 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1167 | 128.115 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1250 | 128.125 | ACC-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 128.1250 | 128.130 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1333 | 128.135 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1417 | 128.140 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1500 | 128.150 | ACC-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 128.1500 | 128.155 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1583 | 128.160 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1667 | 128.165 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1750 | 128.175 | ACC-U | ACC-L, ACC-U | ACC | APP, ACC-L | ACC-L, ACC-U | ACC |
| 128.1750 | 128.180 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1833 | 128.185 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.1917 | 128.190 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2000 | 128.200 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.2000 | 128.205 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2083 | 128.210 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2167 | 128.215 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2250 | 128.225 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.2250 | 128.230 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2333 | 128.235 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2417 | 128.240 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2500 | 128.250 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.2500 | 128.255 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2583 | 128.260 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2667 | 128.265 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2750 | 128.275 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.2750 | 128.280 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2833 | 128.285 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.2917 | 128.290 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3000 | 128.300 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 128.3000 | 128.305 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3083 | 128.310 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3167 | 128.315 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3250 | 128.325 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 128.3250 | 128.330 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3333 | 128.335 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3417 | 128.340 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3500 | 128.350 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 128.3500 | 128.355 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3583 | 128.360 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3667 | 128.365 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3750 | 128.375 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 128.3750 | 128.380 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3833 | 128.385 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.3917 | 128.390 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4000 | 128.400 | ACC-L | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.4000 | 128.405 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4083 | 128.410 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4167 | 128.415 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4250 | 128.425 | ACC-L | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.4250 | 128.430 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4333 | 128.435 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4417 | 128.440 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4500 | 128.450 | ACC-L | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.4500 | 128.455 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4583 | 128.460 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4667 | 128.465 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4750 | 128.475 | ACC-L | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.4750 | 128.480 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4833 | 128.485 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.4917 | 128.490 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5000 | 128.500 | ACC-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 128.5000 | 128.505 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5083 | 128.510 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5167 | 128.515 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5250 | 128.525 | ACC-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 128.5250 | 128.530 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5333 | 128.535 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5417 | 128.540 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5500 | 128.550 | ACC-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 128.5500 | 128.555 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5583 | 128.560 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5667 | 128.565 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5750 | 128.575 | ACC-U | FIS-L, FIS-U | ACC | APP, ACC-L | FIS-L, FIS-U | ACC |
| 128.5750 | 128.580 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5833 | 128.585 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.5917 | 128.590 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6000 | 128.600 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.6000 | 128.605 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6083 | 128.610 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6167 | 128.615 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6250 | 128.625 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.6250 | 128.630 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6333 | 128.635 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6417 | 128.640 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6500 | 128.650 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.6500 | 128.655 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6583 | 128.660 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6667 | 128.665 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6750 | 128.675 | APP-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.6750 | 128.680 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6833 | 128.685 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.6917 | 128.690 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7000 | 128.700 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 128.7000 | 128.705 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7083 | 128.710 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7167 | 128.715 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7250 | 128.725 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 128.7250 | 128.730 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7333 | 128.735 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7417 | 128.740 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7500 | 128.750 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 128.7500 | 128.755 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7583 | 128.760 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7667 | 128.765 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7750 | 128.775 | ACC-U | ACC-L | ACC | APP, ACC-L | ACC-L | ACC |
| 128.7750 | 128.780 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7833 | 128.785 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.7917 | 128.790 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8000 | 128.800 | ACC-U | VOLMET, ATIS | ACC | APP, ACC-L | VOLMET, ATIS | ACC |
| 128.8000 | 128.805 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8083 | 128.810 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8167 | 128.815 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8250 | 128.825 | ACC-U | VOLMET, ATIS | Not allotted | APP, ACC-L | VOLMET, ATIS | Not allotted |
| 128.8250 | 128.830 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8333 | 128.835 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8417 | 128.840 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8500 | 128.850 | ACC-U | VOLMET, ATIS | APP | APP, ACC-L | VOLMET, ATIS | APP |
| 128.8500 | 128.855 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8583 | 128.860 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8667 | 128.865 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8750 | 128.875 | ACC-U | VOLMET, ATIS | APP | APP, ACC-L | VOLMET, ATIS | APP |
| 128.8750 | 128.880 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8833 | 128.885 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.8917 | 128.890 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9000 | 128.900 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 128.9000 | 128.905 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9083 | 128.910 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9167 | 128.915 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9250 | 128.925 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 128.9250 | 128.930 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9333 | 128.935 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9417 | 128.940 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9500 | 128.950 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 128.9500 | 128.955 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9583 | 128.960 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9667 | 128.965 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9750 | 128.975 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 128.9750 | 128.980 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9833 | 128.985 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 128.9917 | 128.990 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0000 | 129.000 | ACC-L | AOC | APP | APP, ACC-L | AOC | APP |
| 129.0000 | 129.005 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0083 | 129.010 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0167 | 129.015 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0250 | 129.025 | ACC-L | AOC | APP | APP, ACC-L | AOC | APP |
| 129.0250 | 129.030 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0333 | 129.035 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0417 | 129.040 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0500 | 129.050 | ACC-L | AOC | APP | APP, ACC-L | AOC | APP |
| 129.0500 | 129.055 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0583 | 129.060 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0667 | 129.065 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0750 | 129.075 | ACC-L | AOC | APP | APP, ACC-L | AOC | APP |
| 129.0750 | 129.080 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0833 | 129.085 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.0917 | 129.090 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1000 | 129.100 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.1000 | 129.105 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1083 | 129.110 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1167 | 129.115 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1250 | 129.125 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.1250 | 129.130 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1333 | 129.135 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1417 | 129.140 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1500 | 129.150 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.1500 | 129.155 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1583 | 129.160 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1667 | 129.165 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1750 | 129.175 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.1750 | 129.180 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1833 | 129.185 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.1917 | 129.190 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2000 | 129.200 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.2000 | 129.205 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2083 | 129.210 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2167 | 129.215 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2250 | 129.225 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.2250 | 129.230 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2333 | 129.235 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2417 | 129.240 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2500 | 129.250 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.2500 | 129.255 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2583 | 129.260 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2667 | 129.265 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2750 | 129.275 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.2750 | 129.280 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2833 | 129.285 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.2917 | 129.290 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3000 | 129.300 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.3000 | 129.305 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3083 | 129.310 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3167 | 129.315 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3250 | 129.325 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.3250 | 129.330 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3333 | 129.335 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3417 | 129.340 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3500 | 129.350 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.3500 | 129.355 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3583 | 129.360 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3667 | 129.365 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3750 | 129.375 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.3750 | 129.380 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3833 | 129.385 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.3917 | 129.390 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4000 | 129.400 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.4000 | 129.405 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4083 | 129.410 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4167 | 129.415 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4250 | 129.425 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.4250 | 129.430 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4333 | 129.435 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4417 | 129.440 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4500 | 129.450 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.4500 | 129.455 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4583 | 129.460 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4667 | 129.465 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4750 | 129.475 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.4750 | 129.480 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4833 | 129.485 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.4917 | 129.490 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5000 | 129.500 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.5000 | 129.505 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5083 | 129.510 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5167 | 129.515 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5250 | 129.525 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.5250 | 129.530 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5333 | 129.535 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5417 | 129.540 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5500 | 129.550 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.5500 | 129.555 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5583 | 129.560 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5667 | 129.565 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5750 | 129.575 | ACC-U | AOC | APP | APP, ACC-L | AOC | APP |
| 129.5750 | 129.580 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5833 | 129.585 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.5917 | 129.590 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6000 | 129.600 | ACC-L | AOC | APP | APP, ACC-L | AOC | APP |
| 129.6000 | 129.605 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6083 | 129.610 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6167 | 129.615 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6250 | 129.625 | ACC-L | AOC | APP | APP, ACC-L | AOC | APP |
| 129.6250 | 129.630 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6333 | 129.635 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6417 | 129.640 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6500 | 129.650 | ACC-L | AOC | APP | APP, ACC-L | AOC | APP |
| 129.6500 | 129.655 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6583 | 129.660 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6667 | 129.665 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6750 | 129.675 | ACC-L | AOC | APP | APP, ACC-L | AOC | APP |
| 129.6750 | 129.680 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6833 | 129.685 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.6917 | 129.690 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 129.7000 | 129.700 | Not allotted | AOC | APP | Not allotted | AOC | APP |
| 129.7000 | 129.705 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.7083 | 129.710 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.7167 | 129.715 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.7250 | 129.725 | Not allotted | AOC | APP | Not allotted | AOC | APP |
| 129.7250 | 129.730 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.7333 | 129.735 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.7417 | 129.740 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.7500 | 129.750 | Not allotted | AOC | APP | Not allotted | AOC | APP |
| 129.7500 | 129.755 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.7583 | 129.760 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.7667 | 129.765 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.7750 | 129.775 | Not allotted | AOC | APP | Not allotted | AOC | APP |
| 129.7750 | 129.780 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.7833 | 129.785 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.7917 | 129.790 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8000 | 129.800 | Not allotted | AOC | APP | Not allotted | AOC | APP |
| 129.8000 | 129.805 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8083 | 129.810 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8167 | 129.815 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8250 | 129.825 | Not allotted | AOC | APP | Not allotted | AOC | APP |
| 129.8250 | 129.830 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8333 | 129.835 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8417 | 129.840 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8500 | 129.850 | Not allotted | AOC | APP | Not allotted | AOC | APP |
| 129.8500 | 129.855 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8583 | 129.860 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8667 | 129.865 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8750 | 129.875 | Not allotted | AOC | Not allotted | Not allotted | AOC | Not allotted |
| 129.8750 | 129.880 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8833 | 129.885 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.8917 | 129.890 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9000 | 129.900 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 129.9000 | 129.905 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9083 | 129.910 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9167 | 129.915 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9250 | 129.925 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 129.9250 | 129.930 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9333 | 129.935 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9417 | 129.940 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9500 | 129.950 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 129.9500 | 129.955 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9583 | 129.960 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9667 | 129.965 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9750 | 129.975 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 129.9750 | 129.980 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9833 | 129.985 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 129.9917 | 129.990 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0000 | 130.000 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.0000 | 130.005 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0083 | 130.010 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0167 | 130.015 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0250 | 130.025 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.0250 | 130.030 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0333 | 130.035 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0417 | 130.040 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0500 | 130.050 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.0500 | 130.055 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0583 | 130.060 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0667 | 130.065 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0750 | 130.075 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.0750 | 130.080 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0833 | 130.085 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.0917 | 130.090 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1000 | 130.100 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.1000 | 130.105 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1083 | 130.110 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1167 | 130.115 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1250 | 130.125 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.1250 | 130.130 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1333 | 130.135 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1417 | 130.140 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1500 | 130.150 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.1500 | 130.155 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1583 | 130.160 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1667 | 130.165 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1750 | 130.175 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.1750 | 130.180 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1833 | 130.185 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.1917 | 130.190 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2000 | 130.200 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.2000 | 130.205 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2083 | 130.210 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2167 | 130.215 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2250 | 130.225 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.2250 | 130.230 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2333 | 130.235 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2417 | 130.240 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2500 | 130.250 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.2500 | 130.255 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2583 | 130.260 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2667 | 130.265 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2750 | 130.275 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.2750 | 130.280 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2833 | 130.285 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.2917 | 130.290 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3000 | 130.300 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.3000 | 130.305 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3083 | 130.310 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3167 | 130.315 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3250 | 130.325 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.3250 | 130.330 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3333 | 130.335 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3417 | 130.340 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3500 | 130.350 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.3500 | 130.355 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3583 | 130.360 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3667 | 130.365 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3750 | 130.375 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.3750 | 130.380 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3833 | 130.385 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.3917 | 130.390 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4000 | 130.400 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.4000 | 130.405 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4083 | 130.410 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4167 | 130.415 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4250 | 130.425 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.4250 | 130.430 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4333 | 130.435 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4417 | 130.440 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4500 | 130.450 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.4500 | 130.455 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4583 | 130.460 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4667 | 130.465 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4750 | 130.475 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.4750 | 130.480 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4833 | 130.485 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.4917 | 130.490 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5000 | 130.500 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.5000 | 130.505 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5083 | 130.510 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5167 | 130.515 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5250 | 130.525 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.5250 | 130.530 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5333 | 130.535 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5417 | 130.540 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5500 | 130.550 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.5500 | 130.555 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5583 | 130.560 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5667 | 130.565 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5750 | 130.575 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.5750 | 130.580 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5833 | 130.585 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.5917 | 130.590 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6000 | 130.600 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.6000 | 130.605 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6083 | 130.610 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6167 | 130.615 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6250 | 130.625 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.6250 | 130.630 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6333 | 130.635 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6417 | 130.640 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6500 | 130.650 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.6500 | 130.655 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6583 | 130.660 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6667 | 130.665 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6750 | 130.675 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.6750 | 130.680 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6833 | 130.685 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.6917 | 130.690 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7000 | 130.700 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.7000 | 130.705 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7083 | 130.710 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7167 | 130.715 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7250 | 130.725 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.7250 | 130.730 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7333 | 130.735 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7417 | 130.740 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7500 | 130.750 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.7500 | 130.755 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7583 | 130.760 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7667 | 130.765 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7750 | 130.775 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.7750 | 130.780 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7833 | 130.785 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.7917 | 130.790 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8000 | 130.800 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.8000 | 130.805 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8083 | 130.810 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8167 | 130.815 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8250 | 130.825 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.8250 | 130.830 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8333 | 130.835 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8417 | 130.840 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8500 | 130.850 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.8500 | 130.855 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8583 | 130.860 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8667 | 130.865 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8750 | 130.875 | Not allotted | AOC | AOC | Not allotted | AOC | AOC |
| 130.8750 | 130.880 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8833 | 130.885 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.8917 | 130.890 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 130.9000 | 130.900 | ACC-U | AOC | AOC | APP, ACC-L | AOC | AOC |
| 130.9000 | 130.905 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 130.9083 | 130.910 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 130.9167 | 130.915 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 130.9250 | 130.925 | ACC-U | AOC | AOC | APP, ACC-L | AOC | AOC |
| 130.9250 | 130.930 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 130.9333 | 130.935 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 130.9417 | 130.940 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 130.9500 | 130.950 | ACC-U | AOC | AOC | APP, ACC-L | AOC | AOC |
| 130.9500 | 130.955 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 130.9583 | 130.960 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 130.9667 | 130.965 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 130.9750 | 130.975 | ACC-U | AOC | AOC | APP, ACC-L | AOC | AOC |
| 130.9750 | 130.980 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 130.9833 | 130.985 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 130.9917 | 130.990 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0000 | 131.000 | Not allotted | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.0000 | 131.005 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0083 | 131.010 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0167 | 131.015 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0250 | 131.025 | Not allotted | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.0250 | 131.030 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0333 | 131.035 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0417 | 131.040 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0500 | 131.050 | Not allotted | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.0500 | 131.055 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0583 | 131.060 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0667 | 131.065 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0750 | 131.075 | Not allotted | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.0750 | 131.080 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0833 | 131.085 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.0917 | 131.090 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1000 | 131.100 | FIS-L | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.1000 | 131.105 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1083 | 131.110 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1167 | 131.115 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1250 | 131.125 | FIS-L | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.1250 | 131.130 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1333 | 131.135 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1417 | 131.140 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1500 | 131.150 | FIS-L | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.1500 | 131.155 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1583 | 131.160 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1667 | 131.165 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1750 | 131.175 | FIS-L | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.1750 | 131.180 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1833 | 131.185 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.1917 | 131.190 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2000 | 131.200 | ACC-L | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.2000 | 131.205 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2083 | 131.210 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2167 | 131.215 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2250 | 131.225 | ACC-L | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.2250 | 131.230 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2333 | 131.235 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2417 | 131.240 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2500 | 131.250 | ACC-L | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.2500 | 131.255 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2583 | 131.260 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2667 | 131.265 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2750 | 131.275 | ACC-L | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.2750 | 131.280 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2833 | 131.285 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.2917 | 131.290 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3000 | 131.300 | FIS-U (GPS) | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.3000 | 131.305 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3083 | 131.310 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3167 | 131.315 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3250 | 131.325 | FIS-U (GPS) | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.3250 | 131.330 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3333 | 131.335 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3417 | 131.340 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3500 | 131.350 | FIS-U (GPS) | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.3500 | 131.355 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3583 | 131.360 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3667 | 131.365 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3750 | 131.375 | FIS-U (GPS) | AOC | AOC | APP, ACC-L | AOC | AOC |
| 131.3750 | 131.380 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3833 | 131.385 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.3917 | 131.390 | Not used | Not used | Not used | APP, ACC-L | Not used | Not used |
| 131.4000 | 131.400 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.4000 | 131.405 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.4083 | 131.410 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.4167 | 131.415 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.4250 | 131.425 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.4250 | 131.430 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.4333 | 131.435 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.4417 | 131.440 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.4500 | 131.450 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.4500 | 131.455 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.4583 | 131.460 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.4667 | 131.465 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.4750 | 131.475 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.4750 | 131.480 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.4833 | 131.485 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.4917 | 131.490 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.5000 | 131.500 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.5000 | 131.505 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.5083 | 131.510 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.5167 | 131.515 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.5250 | 131.525 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.5250 | 131.530 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.5333 | 131.535 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.5417 | 131.540 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.5500 | 131.550 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.5500 | 131.555 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.5583 | 131.560 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.5667 | 131.565 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.5750 | 131.575 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.5750 | 131.580 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.5833 | 131.585 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.5917 | 131.590 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6000 | 131.600 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.6000 | 131.605 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6083 | 131.610 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6167 | 131.615 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6250 | 131.625 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.6250 | 131.630 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6333 | 131.635 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6417 | 131.640 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6500 | 131.650 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.6500 | 131.655 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6583 | 131.660 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6667 | 131.665 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6750 | 131.675 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.6750 | 131.680 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6833 | 131.685 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.6917 | 131.690 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.7000 | 131.700 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.7000 | 131.705 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.7083 | 131.710 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.7167 | 131.715 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.7250 | 131.725 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.7250 | 131.730 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.7333 | 131.735 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.7417 | 131.740 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.7500 | 131.750 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.7500 | 131.755 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.7583 | 131.760 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.7667 | 131.765 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.7750 | 131.775 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.7750 | 131.780 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.7833 | 131.785 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.7917 | 131.790 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.8000 | 131.800 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.8000 | 131.805 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.8083 | 131.810 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.8167 | 131.815 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.8250 | 131.825 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.8250 | 131.830 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.8333 | 131.835 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.8417 | 131.840 | Not used | Not used | Not used | Blocked | Not used | Not used |
| 131.8500 | 131.850 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.8500 | 131.855 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.8583 | 131.860 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.8667 | 131.865 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.8750 | 131.875 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.8750 | 131.880 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.8833 | 131.885 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.8917 | 131.890 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9000 | 131.900 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.9000 | 131.905 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9083 | 131.910 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9167 | 131.915 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9250 | 131.925 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.9250 | 131.930 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9333 | 131.935 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9417 | 131.940 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9500 | 131.950 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.9500 | 131.955 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9583 | 131.960 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9667 | 131.965 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9750 | 131.975 | AOC | AOC | AOC | AOC | AOC | AOC |
| 131.9750 | 131.980 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9833 | 131.985 | Not used | Not used | Not used | AOC | Not used | Not used |
| 131.9917 | 131.990 | Not used | Not used | Not used | AOC | Not used | Not used |
| 132.0000 | 132.000 | Not allotted | AOC | AOC | ACC-U | AOC | AOC |
| 132.0000 | 132.005 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.0083 | 132.010 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.0167 | 132.015 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.0250 | 132.025 | Not allotted | AOC | AOC | ACC-U | AOC | AOC |
| 132.0250 | 132.030 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.0333 | 132.035 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.0417 | 132.040 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.0500 | 132.050 | Not allotted | Not allotted | VOLMET, ATIS | ACC-U | Not allotted | VOLMET, ATIS |
| 132.0500 | 132.055 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.0583 | 132.060 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.0667 | 132.065 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.0750 | 132.075 | Not allotted | Not allotted | VOLMET, ATIS | ACC-U | Not allotted | VOLMET, ATIS |
| 132.0750 | 132.080 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.0833 | 132.085 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.0917 | 132.090 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1000 | 132.100 | ACC-U | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.1000 | 132.105 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1083 | 132.110 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1167 | 132.115 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1250 | 132.125 | ACC-U | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.1250 | 132.130 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1333 | 132.135 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1417 | 132.140 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1500 | 132.150 | ACC-U | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.1500 | 132.155 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1583 | 132.160 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1667 | 132.165 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1750 | 132.175 | ACC-U | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.1750 | 132.180 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1833 | 132.185 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.1917 | 132.190 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2000 | 132.200 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.2000 | 132.205 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2083 | 132.210 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2167 | 132.215 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2250 | 132.225 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.2250 | 132.230 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2333 | 132.235 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2417 | 132.240 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2500 | 132.250 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.2500 | 132.255 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2583 | 132.260 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2667 | 132.265 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2750 | 132.275 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.2750 | 132.280 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2833 | 132.285 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.2917 | 132.290 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3000 | 132.300 | FIS-U (GPS) | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.3000 | 132.305 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3083 | 132.310 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3167 | 132.315 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3250 | 132.325 | FIS-U (GPS) | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.3250 | 132.330 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3333 | 132.335 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3417 | 132.340 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3500 | 132.350 | FIS-U (GPS) | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.3500 | 132.355 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3583 | 132.360 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3667 | 132.365 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3750 | 132.375 | FIS-U (GPS) | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.3750 | 132.380 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3833 | 132.385 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.3917 | 132.390 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4000 | 132.400 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.4000 | 132.405 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4083 | 132.410 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4167 | 132.415 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4250 | 132.425 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.4250 | 132.430 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4333 | 132.435 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4417 | 132.440 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4500 | 132.450 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.4500 | 132.455 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4583 | 132.460 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4667 | 132.465 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4750 | 132.475 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.4750 | 132.480 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4833 | 132.485 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.4917 | 132.490 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5000 | 132.500 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.5000 | 132.505 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5083 | 132.510 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5167 | 132.515 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5250 | 132.525 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.5250 | 132.530 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5333 | 132.535 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5417 | 132.540 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5500 | 132.550 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.5500 | 132.555 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5583 | 132.560 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5667 | 132.565 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5750 | 132.575 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.5750 | 132.580 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5833 | 132.585 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.5917 | 132.590 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6000 | 132.600 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.6000 | 132.605 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6083 | 132.610 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6167 | 132.615 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6250 | 132.625 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.6250 | 132.630 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6333 | 132.635 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6417 | 132.640 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6500 | 132.650 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.6500 | 132.655 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6583 | 132.660 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6667 | 132.665 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6750 | 132.675 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.6750 | 132.680 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6833 | 132.685 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.6917 | 132.690 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7000 | 132.700 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.7000 | 132.705 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7083 | 132.710 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7167 | 132.715 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7250 | 132.725 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.7250 | 132.730 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7333 | 132.735 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7417 | 132.740 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7500 | 132.750 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.7500 | 132.755 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7583 | 132.760 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7667 | 132.765 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7750 | 132.775 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.7750 | 132.780 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7833 | 132.785 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.7917 | 132.790 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8000 | 132.800 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.8000 | 132.805 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8083 | 132.810 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8167 | 132.815 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8250 | 132.825 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.8250 | 132.830 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8333 | 132.835 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8417 | 132.840 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8500 | 132.850 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.8500 | 132.855 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8583 | 132.860 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8667 | 132.865 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8750 | 132.875 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.8750 | 132.880 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8833 | 132.885 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.8917 | 132.890 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9000 | 132.900 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.9000 | 132.905 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9083 | 132.910 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9167 | 132.915 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9250 | 132.925 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.9250 | 132.930 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9333 | 132.935 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9417 | 132.940 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9500 | 132.950 | Not allotted | ACC-L, ACC-U | VOLMET, ATIS | ACC-U | ACC-L, ACC-U | VOLMET, ATIS |
| 132.9500 | 132.955 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9583 | 132.960 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9667 | 132.965 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9750 | 132.975 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 132.9750 | 132.980 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9833 | 132.985 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 132.9917 | 132.990 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0000 | 133.000 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.0000 | 133.005 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0083 | 133.010 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0167 | 133.015 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0250 | 133.025 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.0250 | 133.030 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0333 | 133.035 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0417 | 133.040 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0500 | 133.050 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.0500 | 133.055 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0583 | 133.060 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0667 | 133.065 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0750 | 133.075 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.0750 | 133.080 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0833 | 133.085 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.0917 | 133.090 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1000 | 133.100 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.1000 | 133.105 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1083 | 133.110 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1167 | 133.115 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1250 | 133.125 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.1250 | 133.130 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1333 | 133.135 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1417 | 133.140 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1500 | 133.150 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.1500 | 133.155 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1583 | 133.160 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1667 | 133.165 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1750 | 133.175 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.1750 | 133.180 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1833 | 133.185 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.1917 | 133.190 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2000 | 133.200 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.2000 | 133.205 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2083 | 133.210 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2167 | 133.215 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2250 | 133.225 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.2250 | 133.230 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2333 | 133.235 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2417 | 133.240 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2500 | 133.250 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.2500 | 133.255 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2583 | 133.260 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2667 | 133.265 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2750 | 133.275 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.2750 | 133.280 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2833 | 133.285 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.2917 | 133.290 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3000 | 133.300 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.3000 | 133.305 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3083 | 133.310 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3167 | 133.315 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3250 | 133.325 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.3250 | 133.330 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3333 | 133.335 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3417 | 133.340 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3500 | 133.350 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.3500 | 133.355 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3583 | 133.360 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3667 | 133.365 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3750 | 133.375 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.3750 | 133.380 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3833 | 133.385 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.3917 | 133.390 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4000 | 133.400 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.4000 | 133.405 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4083 | 133.410 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4167 | 133.415 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4250 | 133.425 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.4250 | 133.430 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4333 | 133.435 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4417 | 133.440 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4500 | 133.450 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.4500 | 133.455 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4583 | 133.460 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4667 | 133.465 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4750 | 133.475 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.4750 | 133.480 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4833 | 133.485 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.4917 | 133.490 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5000 | 133.500 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.5000 | 133.505 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5083 | 133.510 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5167 | 133.515 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5250 | 133.525 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.5250 | 133.530 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5333 | 133.535 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5417 | 133.540 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5500 | 133.550 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.5500 | 133.555 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5583 | 133.560 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5667 | 133.565 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5750 | 133.575 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.5750 | 133.580 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5833 | 133.585 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.5917 | 133.590 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6000 | 133.600 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.6000 | 133.605 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6083 | 133.610 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6167 | 133.615 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6250 | 133.625 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.6250 | 133.630 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6333 | 133.635 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6417 | 133.640 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6500 | 133.650 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.6500 | 133.655 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6583 | 133.660 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6667 | 133.665 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6750 | 133.675 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.6750 | 133.680 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6833 | 133.685 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.6917 | 133.690 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7000 | 133.700 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.7000 | 133.705 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7083 | 133.710 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7167 | 133.715 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7250 | 133.725 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.7250 | 133.730 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7333 | 133.735 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7417 | 133.740 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7500 | 133.750 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.7500 | 133.755 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7583 | 133.760 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7667 | 133.765 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7750 | 133.775 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.7750 | 133.780 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7833 | 133.785 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.7917 | 133.790 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8000 | 133.800 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.8000 | 133.805 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8083 | 133.810 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8167 | 133.815 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8250 | 133.825 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.8250 | 133.830 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8333 | 133.835 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8417 | 133.840 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8500 | 133.850 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.8500 | 133.855 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8583 | 133.860 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8667 | 133.865 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8750 | 133.875 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.8750 | 133.880 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8833 | 133.885 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.8917 | 133.890 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9000 | 133.900 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.9000 | 133.905 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9083 | 133.910 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9167 | 133.915 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9250 | 133.925 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.9250 | 133.930 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9333 | 133.935 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9417 | 133.940 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9500 | 133.950 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.9500 | 133.955 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9583 | 133.960 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9667 | 133.965 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9750 | 133.975 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 133.9750 | 133.980 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9833 | 133.985 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 133.9917 | 133.990 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0000 | 134.000 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.0000 | 134.005 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0083 | 134.010 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0167 | 134.015 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0250 | 134.025 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.0250 | 134.030 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0333 | 134.035 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0417 | 134.040 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0500 | 134.050 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.0500 | 134.055 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0583 | 134.060 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0667 | 134.065 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0750 | 134.075 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.0750 | 134.080 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0833 | 134.085 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.0917 | 134.090 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1000 | 134.100 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.1000 | 134.105 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1083 | 134.110 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1167 | 134.115 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1250 | 134.125 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.1250 | 134.130 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1333 | 134.135 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1417 | 134.140 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1500 | 134.150 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.1500 | 134.155 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1583 | 134.160 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1667 | 134.165 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1750 | 134.175 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.1750 | 134.180 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1833 | 134.185 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.1917 | 134.190 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2000 | 134.200 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.2000 | 134.205 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2083 | 134.210 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2167 | 134.215 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2250 | 134.225 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.2250 | 134.230 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2333 | 134.235 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2417 | 134.240 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2500 | 134.250 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.2500 | 134.255 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2583 | 134.260 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2667 | 134.265 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2750 | 134.275 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.2750 | 134.280 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2833 | 134.285 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.2917 | 134.290 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3000 | 134.300 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.3000 | 134.305 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3083 | 134.310 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3167 | 134.315 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3250 | 134.325 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.3250 | 134.330 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3333 | 134.335 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3417 | 134.340 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3500 | 134.350 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.3500 | 134.355 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3583 | 134.360 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3667 | 134.365 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3750 | 134.375 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.3750 | 134.380 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3833 | 134.385 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.3917 | 134.390 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4000 | 134.400 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.4000 | 134.405 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4083 | 134.410 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4167 | 134.415 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4250 | 134.425 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.4250 | 134.430 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4333 | 134.435 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4417 | 134.440 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4500 | 134.450 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.4500 | 134.455 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4583 | 134.460 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4667 | 134.465 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4750 | 134.475 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.4750 | 134.480 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4833 | 134.485 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.4917 | 134.490 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5000 | 134.500 | Not allotted | ACC-L, ACC-U | ACC | ACC-U | ACC-L, ACC-U | ACC |
| 134.5000 | 134.505 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5083 | 134.510 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5167 | 134.515 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5250 | 134.525 | Not allotted | Not allotted | ACC | ACC-U | Not allotted | ACC |
| 134.5250 | 134.530 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5333 | 134.535 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5417 | 134.540 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5500 | 134.550 | Not allotted | Not allotted | ACC | ACC-U | Not allotted | ACC |
| 134.5500 | 134.555 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5583 | 134.560 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5667 | 134.565 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5750 | 134.575 | Not allotted | Not allotted | ACC | ACC-U | Not allotted | ACC |
| 134.5750 | 134.580 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5833 | 134.585 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.5917 | 134.590 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6000 | 134.600 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.6000 | 134.605 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6083 | 134.610 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6167 | 134.615 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6250 | 134.625 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.6250 | 134.630 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6333 | 134.635 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6417 | 134.640 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6500 | 134.650 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.6500 | 134.655 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6583 | 134.660 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6667 | 134.665 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6750 | 134.675 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.6750 | 134.680 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6833 | 134.685 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.6917 | 134.690 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7000 | 134.700 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.7000 | 134.705 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7083 | 134.710 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7167 | 134.715 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7250 | 134.725 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.7250 | 134.730 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7333 | 134.735 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7417 | 134.740 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7500 | 134.750 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.7500 | 134.755 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7583 | 134.760 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7667 | 134.765 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7750 | 134.775 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.7750 | 134.780 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7833 | 134.785 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.7917 | 134.790 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8000 | 134.800 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.8000 | 134.805 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8083 | 134.810 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8167 | 134.815 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8250 | 134.825 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.8250 | 134.830 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8333 | 134.835 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8417 | 134.840 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8500 | 134.850 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.8500 | 134.855 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8583 | 134.860 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8667 | 134.865 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8750 | 134.875 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.8750 | 134.880 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8833 | 134.885 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.8917 | 134.890 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9000 | 134.900 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.9000 | 134.905 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9083 | 134.910 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9167 | 134.915 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9250 | 134.925 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.9250 | 134.930 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9333 | 134.935 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9417 | 134.940 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9500 | 134.950 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.9500 | 134.955 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9583 | 134.960 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9667 | 134.965 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9750 | 134.975 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 134.9750 | 134.980 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9833 | 134.985 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 134.9917 | 134.990 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0000 | 135.000 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.0000 | 135.005 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0083 | 135.010 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0167 | 135.015 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0250 | 135.025 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.0250 | 135.030 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0333 | 135.035 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0417 | 135.040 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0500 | 135.050 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.0500 | 135.055 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0583 | 135.060 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0667 | 135.065 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0750 | 135.075 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.0750 | 135.080 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0833 | 135.085 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.0917 | 135.090 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1000 | 135.100 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.1000 | 135.105 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1083 | 135.110 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1167 | 135.115 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1250 | 135.125 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.1250 | 135.130 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1333 | 135.135 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1417 | 135.140 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1500 | 135.150 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.1500 | 135.155 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1583 | 135.160 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1667 | 135.165 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1750 | 135.175 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.1750 | 135.180 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1833 | 135.185 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.1917 | 135.190 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2000 | 135.200 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.2000 | 135.205 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2083 | 135.210 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2167 | 135.215 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2250 | 135.225 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.2250 | 135.230 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2333 | 135.235 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2417 | 135.240 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2500 | 135.250 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.2500 | 135.255 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2583 | 135.260 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2667 | 135.265 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2750 | 135.275 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.2750 | 135.280 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2833 | 135.285 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.2917 | 135.290 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3000 | 135.300 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.3000 | 135.305 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3083 | 135.310 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3167 | 135.315 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3250 | 135.325 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.3250 | 135.330 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3333 | 135.335 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3417 | 135.340 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3500 | 135.350 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.3500 | 135.355 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3583 | 135.360 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3667 | 135.365 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3750 | 135.375 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.3750 | 135.380 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3833 | 135.385 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.3917 | 135.390 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4000 | 135.400 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.4000 | 135.405 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4083 | 135.410 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4167 | 135.415 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4250 | 135.425 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.4250 | 135.430 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4333 | 135.435 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4417 | 135.440 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4500 | 135.450 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.4500 | 135.455 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4583 | 135.460 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4667 | 135.465 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4750 | 135.475 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.4750 | 135.480 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4833 | 135.485 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.4917 | 135.490 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5000 | 135.500 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.5000 | 135.505 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5083 | 135.510 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5167 | 135.515 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5250 | 135.525 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.5250 | 135.530 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5333 | 135.535 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5417 | 135.540 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5500 | 135.550 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.5500 | 135.555 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5583 | 135.560 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5667 | 135.565 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5750 | 135.575 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.5750 | 135.580 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5833 | 135.585 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.5917 | 135.590 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6000 | 135.600 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.6000 | 135.605 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6083 | 135.610 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6167 | 135.615 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6250 | 135.625 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.6250 | 135.630 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6333 | 135.635 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6417 | 135.640 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6500 | 135.650 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.6500 | 135.655 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6583 | 135.660 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6667 | 135.665 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6750 | 135.675 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.6750 | 135.680 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6833 | 135.685 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.6917 | 135.690 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7000 | 135.700 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.7000 | 135.705 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7083 | 135.710 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7167 | 135.715 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7250 | 135.725 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.7250 | 135.730 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7333 | 135.735 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7417 | 135.740 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7500 | 135.750 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.7500 | 135.755 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7583 | 135.760 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7667 | 135.765 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7750 | 135.775 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.7750 | 135.780 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7833 | 135.785 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.7917 | 135.790 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8000 | 135.800 | Not allotted | FIS-U (GPS) | ACC | ACC-U | FIS-U (GPS) | ACC |
| 135.8000 | 135.805 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8083 | 135.810 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8167 | 135.815 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8250 | 135.825 | Not allotted | Not allotted | ACC | ACC-U | Not allotted | ACC |
| 135.8250 | 135.830 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8333 | 135.835 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8417 | 135.840 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8500 | 135.850 | Not allotted | Not allotted | ACC | ACC-U | Not allotted | ACC |
| 135.8500 | 135.855 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8583 | 135.860 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8667 | 135.865 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8750 | 135.875 | Not allotted | Not allotted | ACC | ACC-U | Not allotted | ACC |
| 135.8750 | 135.880 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8833 | 135.885 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.8917 | 135.890 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9000 | 135.900 | Not allotted | Not allotted | ACC | ACC-U | Not allotted | ACC |
| 135.9000 | 135.905 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9083 | 135.910 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9167 | 135.915 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9250 | 135.925 | Not allotted | Not allotted | ACC | ACC-U | Not allotted | ACC |
| 135.9250 | 135.930 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9333 | 135.935 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9417 | 135.940 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9500 | 135.950 | Not allotted | Not allotted | ACC | ACC-U | Not allotted | ACC |
| 135.9500 | 135.955 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9583 | 135.960 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9667 | 135.965 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9750 | 135.975 | Not allotted | Not allotted | Not allotted | ACC-U | Not allotted | Not allotted |
| 135.9750 | 135.980 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9833 | 135.985 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 135.9917 | 135.990 | Not used | Not used | Not used | ACC-U | Not used | Not used |
| 136.0000 | 136.000 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.0000 | 136.005 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.0083 | 136.010 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.0167 | 136.015 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.0250 | 136.025 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.0250 | 136.030 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.0333 | 136.035 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.0417 | 136.040 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.0500 | 136.050 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.0500 | 136.055 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.0583 | 136.060 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.0667 | 136.065 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.0750 | 136.075 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.0750 | 136.080 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.0833 | 136.085 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.0917 | 136.090 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1000 | 136.100 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.1000 | 136.105 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1083 | 136.110 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1167 | 136.115 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1250 | 136.125 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.1250 | 136.130 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1333 | 136.135 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1417 | 136.140 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1500 | 136.150 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.1500 | 136.155 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1583 | 136.160 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1667 | 136.165 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1750 | 136.175 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.1750 | 136.180 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1833 | 136.185 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.1917 | 136.190 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2000 | 136.200 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.2000 | 136.205 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2083 | 136.210 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2167 | 136.215 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2250 | 136.225 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.2250 | 136.230 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2333 | 136.235 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2417 | 136.240 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2500 | 136.250 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.2500 | 136.255 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2583 | 136.260 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2667 | 136.265 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2750 | 136.275 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.2750 | 136.280 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2833 | 136.285 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.2917 | 136.290 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3000 | 136.300 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.3000 | 136.305 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3083 | 136.310 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3167 | 136.315 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3250 | 136.325 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.3250 | 136.330 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3333 | 136.335 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3417 | 136.340 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3500 | 136.350 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.3500 | 136.355 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3583 | 136.360 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3667 | 136.365 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3750 | 136.375 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.3750 | 136.380 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3833 | 136.385 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.3917 | 136.390 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.4000 | 136.400 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.4000 | 136.405 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.4083 | 136.410 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.4167 | 136.415 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.4250 | 136.425 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.4250 | 136.430 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.4333 | 136.435 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.4417 | 136.440 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.4500 | 136.450 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
| 136.4500 | 136.455 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.4583 | 136.460 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.4667 | 136.465 | Not used | Not used | Not used | Not allotted | Not used | Not used |
| 136.4750 | 136.475 | Not allotted | VDL | Not allotted | Not allotted | Not allotted | Not allotted |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.5000 | 136.500 | VDL=guard | VDL=guard | VDL--guard | VDL-guard | VDL-guard | VDL-guard |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.5250 | 136.525 | VDL | VDL | VDL | VDL | VDL | VDL |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.5500 | 136.550 | VDL=guard | VDL=guard | VDL--guard | VDL-guard | VDL-guard | VDL-guard |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.5750 | 136.575 | VDL | VDL | VDL | VDL | VDL | VDL |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.6000 | 136.600 | VDL=guard | VDL=guard | VDL--guard | VDL-guard | VDL-guard | VDL-guard |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.6250 | 136.625 | VDL | VDL | VDL | VDL | VDL | VDL |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.6500 | 136.650 | VDL=guard | VDL=guard | VDL--guard | VDL-guard | VDL-guard | VDL-guard |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.6750 | 136.675 | VDL | VDL | VDL | VDL | VDL | VDL |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.7000 | 136.700 | VDL=guard | VDL=guard | VDL--guard | VDL-guard | VDL-guard | VDL-guard |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.7250 | 136.725 | VDL | VDL | VDL | VDL | VDL | VDL |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.7500 | 136.750 | VDL=guard | VDL=guard | VDL--guard | VDL-guard | VDL-guard | VDL-guard |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.7750 | 136.775 | VDL | VDL | VDL | VDL | VDL | VDL |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.8000 | 136.800 | VDL=guard | VDL=guard | VDL--guard | VDL-guard | VDL-guard | VDL-guard |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.8250 | 136.825 | VDL | VDL | VDL | VDL | VDL | VDL |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.8500 | 136.850 | VDL=guard | VDL=guard | VDL--guard | VDL-guard | VDL-guard | VDL-guard |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.8750 | 136.875 | VDL | VDL | VDL | VDL | VDL | VDL |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.9000 | 136.900 | VDL=guard | VDL=guard | VDL--guard | VDL-guard | VDL-guard | VDL-guard |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.9250 | 136.925 | VDL | VDL | VDL | VDL | VDL | VDL |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.9500 | 136.950 | VDL=guard | VDL=guard | VDL--guard | VDL-guard | VDL-guard | VDL-guard |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| 136.9750 | 136.975 | VDL | VDL | VDL | VDL | VDL | VDL |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |